{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["检验结果汇总表"],"not_rendered":{"external_links":1,"defined_names":2,"comments":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"检验结果汇总表","index":0,"n_rows":12,"n_cols":15,"rows_kept":12,"merged":[[0,0,0,14]],"flags":["formulas_cached_only"]}
["2023年水泥产品质量监督抽查检验结果汇总表"]
["序号","产品名称\n（商品实物标注名称）","标称商标\n（有TM标记，或注册商标R标记的）","生产日期/批号","规格型号","抽样日期","受检单位","受检单位信用代码","受检单位地址","标称生产单位","标称生产单位地址","检查内容\n（主要检验项目）","检验结果判定","不合格项目","承检机构名称"]
[1,"水泥","——","2023.5.6","P.C 42.5","2023-05-12","江阴市华西水泥有限公司","913202817494104906","江阴市华士镇华西工业园区中康路","——","——","抗折强度(P.C/P.F/P.P/P.S.A/P.S.B)、抗压强度(P.C/P.F/P.P/P.S.A/P.S.B)、凝结时间、安定性、氯离子，%、三氧化硫，%、氧化镁，%、放射性核素限量","合格","_","苏州市产品质量监督检验院"]
[2,"水泥","绮星","2023.5.6","P.O 42.5","2023-05-11","江阴绮星水泥有限公司","91320281142225264B","江阴市云亭街道定山村小山头218号","——","——","抗折强度(P.O/P.Ⅰ/P.Ⅱ)、抗压强度(P.O/P.Ⅰ/P.Ⅱ)、凝结时间、安定性、氯离子，%、三氧化硫，%、氧化镁，%、烧失量，%、放射性核素限量","合格","_","苏州市产品质量监督检验院"]
[3,"水泥","——","2023.5.8","P.C 42.5","2023-05-11","江苏金峰月城水泥有限公司","9132028169454866XU","江阴市月城镇环山路21号","——","——","抗折强度(P.C/P.F/P.P/P.S.A/P.S.B)、抗压强度(P.C/P.F/P.P/P.S.A/P.S.B)、凝结时间、安定性、氯离子，%、三氧化硫，%、氧化镁，%、放射性核素限量","合格","_","苏州市产品质量监督检验院"]
[4,"水泥","——","——","M 32.5","2023-05-12","江阴秀哥建材有限公司","91320281MA269PX46T","江阴市周庄镇金湾村庙头10-3号","无锡市天裕建材有限公司","江苏省无锡市宜兴市芳桥街道工业集中区屺扶路","氯离子，%、三氧化硫，%、细度，%、凝结时间、安定性、保水率，%、抗压强度(32.5)、抗折强度(32.5)、放射性核素限量、水泥中水溶性六价铬","合格","_","苏州市产品质量监督检验院"]
[5,"水泥","——","——","M 32.5","2023-05-12","江阴市周庄小宋水泥店","92320281MA1WCBTLXH","江阴市周庄镇宗言村东门楼下38号-1","无锡市金久水泥有限公司","江苏省无锡市宜兴市屺亭街道袁桥路20号","氯离子，%、三氧化硫，%、细度，%、凝结时间、安定性、保水率，%、抗压强度(32.5)、抗折强度(32.5)、放射性核素限量、水泥中水溶性六价铬","合格","_","苏州市产品质量监督检验院"]
[6,"水泥","绮星","——","P⋅F 32.5","2023-05-23","江阴市申港成涛建材经营部","92320281MA1R835T4J","江阴市镇澄路1649号","江阴绮星水泥有限公司","江苏省无锡市江阴市云亭街道定山村小山头218号","凝结时间、安定性、氯离子，%、三氧化硫，%、氧化镁，%、放射性核素限量、抗折强度(P.F/P.P/P.S.A/P.S.B)、抗压强度(P.F/P.P/P.S.A/P.S.B)","合格","_","苏州市产品质量监督检验院"]
[7,"水泥","东一","——","M 32.5","2023-05-24","江阴市满兴建材经营部","92320281MA1QYA9375","江阴市南闸街道锡澄路299号","宜兴市东一建材有限公司","江苏省无锡市宜兴市徐舍镇美栖村","氯离子，%、三氧化硫，%、细度，%、凝结时间、安定性、保水率，%、抗压强度(32.5)、抗折强度(32.5)、放射性核素限量、水泥中水溶性六价铬","合格","_","苏州市产品质量监督检验院"]
[8,"水泥","——","——","M 32.5","2023-06-06","江阴秀哥建材有限公司","91320281MA269PX46T","江阴市周庄镇金湾村庙头10-3号","无锡市天裕建材有限公司","江苏省无锡市宜兴市芳桥街道工业集中区屺扶路","氯离子，%、三氧化硫，%、细度，%、凝结时间、安定性、保水率，%、抗压强度(32.5)、抗折强度(32.5)、放射性核素限量、水泥中水溶性六价铬","合格","_","苏州市产品质量监督检验院"]
[9,"水泥","——","——","M 32.5","2023-06-06","江阴市周庄小宋水泥店","92320281MA1WCBTLXH","江阴市周庄镇宗言村东门楼下38号-1","无锡市金久水泥有限公司","江苏省无锡市宜兴市屺亭街道袁桥路20号","氯离子，%、三氧化硫，%、细度，%、凝结时间、安定性、保水率，%、抗压强度(32.5)、抗折强度(32.5)、放射性核素限量、水泥中水溶性六价铬","合格","_","苏州市产品质量监督检验院"]
[10,"水泥","绮星","——","P⋅F 32.5","2023-06-06","江阴市满兴建材经营部","92320281MA1QYA9375","江阴市南闸街道锡澄路299号","江阴绮星水泥有限公司","江苏省无锡市江阴市云亭街道定山村小山头218号","凝结时间、安定性、氯离子，%、三氧化硫，%、氧化镁，%、放射性核素限量、抗折强度(P.F/P.P/P.S.A/P.S.B)、抗压强度(P.F/P.P/P.S.A/P.S.B)","合格","_","苏州市产品质量监督检验院"]