{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":37,"n_cols":10,"rows_kept":37,"merged":[[0,0,0,9],[1,0,1,3],[1,8,1,9],[35,0,35,1],[35,8,35,9],[36,0,36,9]],"flags":["formulas_cached_only"]}
["2020年流通领域商品质量抽查检验结果汇总表"]
["填报单位：温州市质量技术检测科学研究院",{"$nulls":7},"填报时间：2020-12-8"]
["序号","报告编号","样品名称","被抽查检验经营者","标称商标","标称生产者","规格/型号","生产日期/批号","综合判定（合格/不合格）","主要不合格项目"]
[1,"NLKF20100152","室内照明开关[二开(双控开关)]","温州市瓯海新桥王红五金店","TCLIOIFGICNB","重庆罗恪朗电器有限公司(标称)","2K2   16AX 250V～",null,"不合格","标志"]
[2,"NLKF20100199","暗装跷板式双控开关","叶祥林","群邦","温州品耐德电气有限公司(标称)","NO.CX1/2   10AX 250V～",null,"不合格","标志"]
[3,"NLKF20100207","暗装跷板式双控开关","永嘉县江北雅居仕装潢批发部","龙洋","温州市龙洋电器有限公司(标称)","  10AX 250V～","2019-3","不合格","标志"]
[4,"NLKF20100209","二位暗装跷板式双控开关","永嘉县江北雅居仕装潢批发部",null,"温州天欧电气有限公司(标称)"," NO.FT1/04   10AX 250V～",null,"不合格","标志、耐热"]
[5,"NLKF20100221","室内照明开关(二开双控开关)","乐清市柳市力玺五金店","图形商标","上海人民电器开关厂集团有限公司(标称)","A系列   10AX 250V～",null,"不合格","标志"]
[6,"NLKF20100225","照明开关(一位双控开关)","乐清市彤彤电气经营部",null,"上海德力西开关有限公司(标称)","DC86D10H系列   16X 250V～","2020.7.11","不合格","标志"]
[7,"NLKF20100275","一开双控开关","苍南县泰蒙五金店",null,"深圳尚品美家电器有限公司(标称)","E6 灰(拉扣式)  10AX  250V～",null,"不合格","标志"]
[8,"NLKF20100276","二开双控开关","苍南县泰蒙五金店",null,"深圳尚品美家电器有限公司(标称)","E6 灰(拉扣式)  10AX  250V～",null,"不合格","标志"]
[9,"NLKF20100294","二位暗装跷板式双控开关","瑞安市塘下丽光水暖器材店",null,"瑞安市帝王电器有限公司(标称)","C12 10AX  250V～",null,"不合格","标志"]
[10,"NLKF20100296","暗装跷板式双控开关","瑞安市塘下金春五金交电经营部",null,"宁波欧美光源科技有限公司(标称)","1K2  10AX  250V～",null,"不合格","标志"]
[11,"NLKF20100303","暗装跷板式双控开关","平阳县林孔喜五金店",null,"阜阳市双燕电器有限公司(标称)"," 16A  250V～",null,"不合格","标志、爬电距离、电气间隙和穿通密封胶距离"]
[12,"NLKF20100307","暗装跷板式双控开关","平阳县阿超灯具店",null,"深圳市豪顿国际照明电器有限公司(标称)","G2   10AX  250V～",null,"不合格","标志"]
[13,"NLKF20100374","暗装跷板式双控开关","温州广纳五金装饰市场陈彩玉五金店","沃克仕","温州虹胜电器有限公司(标称)","LJ.101(2)  10AX  250V～","2020-9-3","不合格","标志"]
[14,"NLKF20100139","一联双控开关","温州市瓯海娄桥国微五金店","CHNT","浙江正泰建筑电器有限公司(标称)","NEW7-E00200A  10AX 250V～",null,"合格"]
[15,"NLKF20100142","一位跷板式双控开关","温州市鹿城区蒲鞋市朱德华电器店",null,"施耐德电气（中国）有限公司(标称)","A3G31_2A   10AX 250V～","2019.10.12","合格"]
[16,"NLKF20100145","单联双控大跷板开关","温州市鹿城区蒲鞋市朱德华电器店",null,"豪意电器科技有限公司(标称)","HY86K12   16AX 250V～",null,"合格"]
[17,"NLKF20100150","照明开关(二位暗装跷板式双控开关)","温州市瓯海娄桥阿靖五金店",null,"泰力实业有限公司(标称)","86GC02-2   10AX 250V～",null,"合格"]
[18,"NLKF20100151","照明开关(二位双控开关)","温州市瓯海娄桥阿靖五金店","凯立德","深圳凯立德照明有限公司(标称)","2K2   10AX 250V～","2020.5.26","合格"]
[19,"NLKF20100219","照明开关(一开双控开关)","乐清市柳市力玺五金店",null,"上海人民电器开关厂集团有限公司(标称)","RM-A002   10AX 250V～",null,"合格"]
[20,"NLKF20100226","室内照明开关(一开双控)","乐清市彤彤电气经营部",null,"浙江开际电气有限公司(标称)","1K2   10AX 250V～",null,"合格"]
[21,"NLKF20100261","三位双控带荧光开关","苍南县灵溪旺盛五金店",null,"宁波公牛电器有限公司(标称)","G32K312  10AX  250V～","2019/10/17","合格"]
[22,"NLKF20100262","照明开关(二位双控带荧光开关)","苍南县铭佳五金经营部",null,"公牛集团宁波公牛电器有限公司(标称)","G28K212CU18  16AX  250V～","2020.4.6","合格"]
[23,"NLKF20100297","二位暗装跷板式双控开关","瑞安市塘下金春五金交电经营部",null,"厦门视贝科技有限公司(标称)","Q1-122  10AX  250V～",null,"合格"]
[24,"NLKF20100300","暗装跷板式双控开关","温州鑫麦建材装饰有限公司",null,"龙胜电器有限公司(标称)","E65N1112F  10AX  250V～",null,"合格"]
[25,"NLKF20100302","二位暗装跷板式双控开关","温州鑫麦建材装饰有限公司","legrand","TCL—罗格朗国际电工（惠州）有限公司(标称)","K8/32/2/3C-C3  16AX  250V～",null,"合格"]
[26,"NLKF20100308","暗装跷板式双控开关","平阳县先君建材经营部","美好","深圳瑞威电器有限公司(标称)","MH-12   10AX  250V～","2019-05-22","合格"]
[27,"NLKF20100311","一位双控开关功能件","苍南县龙港南方五金装璜店","飞雕","飞雕电器集团有限公司(标称)","Q3-Q1/2   10AX  250V～",null,"合格"]
[28,"NLKF20100313","暗装跷板式双控开关","温州五金城金牛灯饰店",null,"欧普照明电器（中山）有限公司(标称)","W171012A-H3  10AX  250V～","2020.04.07","合格"]
[29,"NLKF20100376","暗装跷板式双控开关","温州广纳五金装饰市场义新卫生洁具店",null,"上海彤晶电气有限公司(标称)","NO.ML1/02  10AX  250V～","2019-11","合格"]
[30,"NLKF20110196","联体支架一位双控开关","苍南县泰宇建材有限公司","飞雕","飞雕电器集团有限公司(标称)","E5-A10Q1/2-L   10AX  250V～",null,"合格"]
[31,"NLKF20110198","一位双控开关功能件带按键","苍南县泰宇建材有限公司",null,"飞雕电器集团有限公司(标称)","GDLW-16Q1/2 双控  16AX  250V～",null,"合格"]
[]
["联系人： 王法",{"$nulls":7},"联系电话：0577-89782278"]
["注：综合判定结果依据检验报告填写合格或者不合格，综合判定为不合格的商品需填写主要不合格项目。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}