{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["检验结果汇总表"],"not_rendered":{"external_links":1,"defined_names":2,"comments":3},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"检验结果汇总表","index":0,"n_rows":22,"n_cols":15,"rows_kept":22,"merged":[[0,0,0,14]],"flags":["formulas_cached_only"]}
["2023年涂料产品质量监督抽查检验结果汇总表"]
["序号","产品名称\n（商品实物标注名称）","标称商标\n（有TM标记，或注册商标R标记的）","生产日期/批号","规格型号","抽样日期","受检单位","受检单位信用代码","受检单位地址","标称生产单位","标称生产单位地址","检查内容\n（主要检验项目）","检验结果判定","不合格项目","承检机构名称"]
[1,"雅时利内墙乳胶漆（高遮盖）","_","2023年2月17日","20kg/桶","2023-05-11","江阴市南闸时代装璜商店","320281600005395","江阴市南闸镇南焦路57号","雅士利涂料(苏州)有限公司","苏州工业园区东宏路48号","挥发性有机化合物含量、苯系物总和(苯、甲苯、二甲苯(含乙苯))、甲醛、总铅、可溶性重金属、低温稳定性(3次循环)、低温成膜性、干燥时间(表干)、耐碱性(24h)、抗泛碱性(48h)、对比率、耐洗刷性，次","合格","_","苏州市产品质量监督检验院"]
[2,"美得丽内墙乳胶漆","_","2022年10月14日","5升/桶","2023-05-11","江阴市南闸胖胖建材店","320281600963243","江阴市南闸街道南焦路39号","立邦装饰材料(广州)有限公司","广东省广州市黄埔区（中新广州知识城）亿创街2号916房","挥发性有机化合物含量、苯系物总和(苯、甲苯、二甲苯(含乙苯))、甲醛、总铅、可溶性重金属、低温稳定性(3次循环)、低温成膜性、干燥时间(表干)、耐碱性(24h)、抗泛碱性(48h)、对比率、耐洗刷性，次","合格","_","苏州市产品质量监督检验院"]
[3,"酚醛防腐涂料 中黄","图形商标","2023年2月21日","3kg/桶","2023-05-11","江阴市徐霞客国庆建材商店","92320281MA1R4KQQ8D","江阴市徐霞客镇璜塘教师新村16幢102室","无锡市造漆厂有限公司","江阴市祝塘镇工业园区（西区）金昌路7号","容器中状态、结皮性、施工性、涂膜外观、柔韧性，mm、耐水性(8h)、干燥时间、细度、不挥发物含量，%、流出时间(ISO6号杯)，s","合格","_","苏州市产品质量监督检验院"]
[4,"中灰防锈高闪点安全型醇酸涂料","吉人","2022年12月07日","2kg/桶","2023-05-11","江阴市徐霞客庄臣建材店","92320281MA1R23CM96","江阴市徐霞客镇璜塘环东路43号","苏州吉人高新材料股份有限公司","苏州市相城区黄埭镇春旺路18号","不挥发物含量，%、流出时间(ISO6号杯)，s、干燥时间、弯曲试验、细度、遮盖力、光泽(60°)、硬度、划格试验，级","合格","_","苏州市产品质量监督检验院"]
[5,"经济型哑光内墙乳胶漆","图形商标","2023.3.1","10kg/桶","2023-05-11","无锡市造漆厂有限公司","91320281135890434M","江苏省无锡市江阴市祝塘镇工业园区（西区）金昌路7号","_","_","挥发性有机化合物含量、苯系物总和(苯、甲苯、二甲苯(含乙苯))、甲醛、总铅、可溶性重金属、低温稳定性(3次循环)、低温成膜性、干燥时间(表干)、耐碱性(24h)、抗泛碱性(48h)、对比率、耐洗刷性，次","合格","_","苏州市产品质量监督检验院"]
[6,"纯净界贝白净味墙面漆","三棵树","2022年6月23日","24kg/桶","2023-05-12","江阴市云亭街道三棵树油漆店","92320281MA25HMMB8L","江阴市云亭街道云顾路134号","安徽三棵树涂料有限公司","安徽省明光市化工集中区经四路1号","挥发性有机化合物含量、苯系物总和(苯、甲苯、二甲苯(含乙苯))、甲醛、总铅、可溶性重金属、低温稳定性(3次循环)、低温成膜性、干燥时间(表干)、耐碱性(24h)、抗泛碱性(48h)、对比率、耐洗刷性，次","合格","_","苏州市产品质量监督检验院"]
[7,"白涂料","_","2023.5.23","_","2023-05-23","江阴市恒源涂料有限公司","91320281739572584L","江阴市南闸镇工业园","_","_","VOC含量、乙二醇醚及醚酯总和含量(限乙二醇甲醚、乙二醇甲醚醋酸酯、乙二醇乙醚、乙二醇乙醚醋酸酯、乙二醇二甲醚、乙二醇二乙醚、二乙二醇二甲醚、三乙二醇二甲醚)、重金属含量","合格","_","苏州市产品质量监督检验院"]
[8,"氨基树脂类涂料","_","2023.5.24","18kg/桶","2023-05-24","江阴华理防腐涂料有限公司","91320281607981239T","江苏省江阴市璜土镇立埭村","_","_","VOC含量、乙二醇醚及醚酯总和含量(限乙二醇甲醚、乙二醇甲醚醋酸酯、乙二醇乙醚、乙二醇乙醚醋酸酯、乙二醇二甲醚、乙二醇二乙醚、二乙二醇二甲醚、三乙二醇二甲醚)、重金属含量","合格","_","苏州市产品质量监督检验院"]
[9,"清漆","_","2023.05.22","P-2709","2023-05-24","江阴市荣新塑化有限公司","91320281250417351K","江阴市石庄私营工业园区兴隆路5号","_","_","挥发性有机化合物含量、苯、甲苯、乙苯和二甲苯、乙二醇甲醚、乙二醇乙醚、乙二醇甲醚醋酸酯、乙二醇乙醚醋酸酯、二乙二醇丁醚醋酸酯总量","合格","_","苏州市产品质量监督检验院"]
[10,"丙烯酸酯类树脂涂料","_","2023.5.15","丙烯酸酯白漆","2023-05-25","江阴市欧可化工涂料有限公司","913202817514409203","江阴市顾山镇鉴青村朱家坝2号","_","_","VOC含量、苯含量、甲苯与二甲苯(含乙苯)总和含量、卤代烃总和含量(限二氯甲烷、三氯甲烷、四氯化碳、１，１-二氯乙烷、１，２-二氯乙烷、１，１，１-三氯乙烷、１，１，２-三氯乙烷、１，２-二氯丙烷、１，２，３-三氯丙烷、三氯乙烯、四氯乙烯)、多环芳烃总和含量(限萘、蒽)、乙二醇醚及醚酯总和含量(限乙二醇甲醚、乙二醇甲醚醋酸酯、乙二醇乙醚、乙二醇乙醚醋酸酯、乙二醇二甲醚、乙二醇二乙醚、二乙二醇二甲醚、三乙二醇二甲醚)、重金属含量","合格","_","苏州市产品质量监督检验院"]
[11,"食品罐头专用环氧酚醛树脂涂料","_","2023.5.21","_","2023-05-25","江阴市兴国食品包装涂料有限公司","91320281250347250F","江阴市顾山镇鉴青村","_","_","VOC含量、苯含量、甲苯与二甲苯(含乙苯)总和含量、卤代烃总和含量(限二氯甲烷、三氯甲烷、四氯化碳、１，１-二氯乙烷、１，２-二氯乙烷、１，１，１-三氯乙烷、１，１，２-三氯乙烷、１，２-二氯丙烷、１，２，３-三氯丙烷、三氯乙烯、四氯乙烯)、多环芳烃总和含量(限萘、蒽)、乙二醇醚及醚酯总和含量(限乙二醇甲醚、乙二醇甲醚醋酸酯、乙二醇乙醚、乙二醇乙醚醋酸酯、乙二醇二甲醚、乙二醇二乙醚、二乙二醇二甲醚、三乙二醇二甲醚)、重金属含量","合格","_","苏州市产品质量监督检验院"]
[12,"粉末涂料 S9652HG","精博","2023.5.25","_","2023-05-25","江阴市博泰高分子材料有限公司","91320281728691705D","江阴市顾山镇锡张路166号","_","_","VOC含量、苯含量、甲苯与二甲苯(含乙苯)总和含量、卤代烃总和含量(限二氯甲烷、三氯甲烷、四氯化碳、１，１-二氯乙烷、１，２-二氯乙烷、１，１，１-三氯乙烷、１，１，２-三氯乙烷、１，２-二氯丙烷、１，２，３-三氯丙烷、三氯乙烯、四氯乙烯)、多环芳烃总和含量(限萘、蒽)、乙二醇醚及醚酯总和含量(限乙二醇甲醚、乙二醇甲醚醋酸酯、乙二醇乙醚、乙二醇乙醚醋酸酯、乙二醇二甲醚、乙二醇二乙醚、二乙二醇二甲醚、三乙二醇二甲醚)、重金属含量","合格","_","苏州市产品质量监督检验院"]
[13,"环氧防锈底漆","_","2023.02.28","17L/桶","2023-05-25","江阴市大阪涂料有限公司","91320281250415583R","江阴市顾山镇西朱家巷","_","_","在容器中状态、干燥时间、附着力、不挥发分，%、耐冲击性、挥发性有机化合物(VOC)、苯含量、甲苯与二甲苯(含乙苯)总和含量、卤代烃总和含量(限二氯甲烷、三氯甲烷、四氯化碳、１，１-二氯乙烷、１，２-二氯乙烷、１，１，１-三氯乙烷、１，１，２-三氯乙烷、１，２-二氯丙烷、１，２，３-三氯丙烷、三氯乙烯、四氯乙烯)、多环芳烃总和含量(限萘、蒽)、乙二醇醚及醚酯总和含量(限乙二醇甲醚、乙二醇甲醚醋酸酯、乙二醇乙醚、乙二醇乙醚醋酸酯、乙二醇二甲醚、乙二醇二乙醚、二乙二醇二甲醚、三乙二醇二甲醚)、重金属含量","合格","_","苏州市产品质量监督检验院"]
[14,"环氧底漆","_","2023.5.25","7353灰","2023-05-25","无锡市玉邦树脂涂料有限公司","91320281750047908U","江阴市徐霞客镇马镇北渚村南绛237号","_","_","在容器中状态、干燥时间、附着力、不挥发分，%、耐冲击性、挥发性有机化合物(VOC)、苯含量、甲苯与二甲苯(含乙苯)总和含量、卤代烃总和含量(限二氯甲烷、三氯甲烷、四氯化碳、１，１-二氯乙烷、１，２-二氯乙烷、１，１，１-三氯乙烷、１，１，２-三氯乙烷、１，２-二氯丙烷、１，２，３-三氯丙烷、三氯乙烯、四氯乙烯)、多环芳烃总和含量(限萘、蒽)、乙二醇醚及醚酯总和含量(限乙二醇甲醚、乙二醇甲醚醋酸酯、乙二醇乙醚、乙二醇乙醚醋酸酯、乙二醇二甲醚、乙二醇二乙醚、二乙二醇二甲醚、三乙二醇二甲醚)、重金属含量","合格","_","苏州市产品质量监督检验院"]
[15,"大红高闪点低VOC醇酸防护涂料（高光）","冠军漆","2022年01月22日","600g/桶","2023-06-13","江阴市锐云装饰工程有限公司","91320281MA21G5UE87","江阴市永康五金城八街10-12号","江苏冠军科技集团股份有限公司","江苏省南京市溧水区洪蓝镇工业园","不挥发物含量，%、流出时间(ISO6号杯)，s、干燥时间、弯曲试验、细度、遮盖力、光泽(60°)、硬度、划格试验，级","合格","_","苏州市产品质量监督检验院"]
[16,"家丽安（新）白漆","多乐士","2022年10月25日","18L/桶","2023-06-13","江阴市城区兰嘉建材商行","92320281MA21N8666J","江阴市五金八街42、44号","阿克苏诺贝尔漆油（上海）有限公司","上海市松江工业区荣乐东路536号","低温稳定性(3次循环)、低温成膜性、干燥时间(表干)、耐碱性(24h)、抗泛碱性(48h)、对比率、耐洗刷性，次、挥发性有机化合物含量、苯系物总和(苯、甲苯、二甲苯(含乙苯))、甲醛、总铅、可溶性重金属","合格","_","苏州市产品质量监督检验院"]
[17,"大红醇酸亮光面漆","红业","2023年1月31日","15kg/桶","2023-06-13","江阴市澄江街道晶金装饰材料经营部","92320281MA259R4A5Q","江阴市永康大街119号","上海即缘化工科技有限公司","上海市奉贤区联合北路215号第1幢3171室","不挥发物含量，%、流出时间(ISO6号杯)，s、干燥时间、细度、遮盖力、光泽(60°)、硬度、划格试验，级","合格","_","苏州市产品质量监督检验院"]
[18,"多功能水性装饰漆","岩壁水漆","2023年4月12日","2.5kg/桶","2023-06-14","江阴市恒浩建材商行","92320281MAC5XF9D82","无锡市江阴市黄龙路19号","岩壁（上海）涂料有限公司","上海市嘉定区马陆工业区博学路138号","VOC含量、乙二醇醚及醚酯总和含量(限乙二醇甲醚、乙二醇甲醚醋酸酯、乙二醇乙醚、乙二醇乙醚醋酸酯、乙二醇二甲醚、乙二醇二乙醚、二乙二醇二甲醚、三乙二醇二甲醚)、重金属含量","合格","_","苏州市产品质量监督检验院"]
[19,"竹炭伏饰家无添加二合一内墙漆","华润漆","2021年4月25日","18L/桶","2023-06-14","江阴市雅美墙纸经营部","92320281MA1R30BY8Q","江阴市澄南一村2幢103室","威士伯涂料（广东）有限公司","广东省佛山市顺德区顺番公路五沙段7号之一","低温稳定性(3次循环)、低温成膜性、干燥时间(表干)、耐碱性(24h)、抗泛碱性(48h)、对比率、耐洗刷性，次、挥发性有机化合物含量、苯系物总和(苯、甲苯、二甲苯(含乙苯))、甲醛、总铅、可溶性重金属","合格","_","苏州市产品质量监督检验院"]
[20,"尚享CJ500墙面漆","图形商标","2023.03.11","15L/桶","2023-06-14","江阴市要塞大拇指油漆辅助工具商行","92320281MA21W1YQ8F","江阴市环城南路488、490、492号","杭州德爱威云建材科技有限公司","浙江省杭州市建德市下涯镇马目路11号","低温稳定性(3次循环)、低温成膜性、干燥时间(表干)、耐碱性(24h)、抗泛碱性(48h)、对比率、耐洗刷性，次、挥发性有机化合物含量、苯系物总和(苯、甲苯、二甲苯(含乙苯))、甲醛、总铅、可溶性重金属","合格","_","苏州市产品质量监督检验院"]